=============================================================================

  (c) SYSTEC electronic GmbH, D-08468 Heinsdorfergrund, Am Windrad 2
      www.systec-electronic.com

  Product:      3912003 - IoT-Chip Utility Package

=============================================================================



This package contains the following components:


 3912003 - IoT-Chip Utility Package
  |
  + IoT-Chip Examples
  |   |
  |   +- I2c_Lcd_Driver
  |   |     OpenPCS / PLC sample project
  |   |     Topic: How to print text on a LCD display using the I2C FB Library
  |   |
  |   +- IoTChip_RFID_LCD
  |   |     OpenPCS / PLC sample project
  |   |     Topic: How to read a RFID tag and print its number on a LCD
  |   |
  |   +- IoTChip_RFID_LCD_MQTT_Oublish
  |   |     OpenPCS / PLC sample project
  |   |     Topic: How to read a RFID tag, print its number on a LCD and publish
  |   |            its tag number via MQTT to a broker server
  |   |            (needs 'Mosquitto_Server', see below)
  |   |
  |   +- Mosquitto_Server
  |   |     MQTT broker server 'Mosquitto', needed for OpenPCS / PLC sample project
  |   |     'IoTChip_RFID_LCD_MQTT' (see above)
  |   |     PLEASE NOTE 'LICENSE.txt' inside this application folder
  |   |
  |   +- Schematic_IoT-RFID-LCD.png
  |   |     Schematic for connecting RFID Reader and LCD Display to the IoT-Chip
  |   |
  |   +- IoT-RFID-LCD.jpg
  |   |     Real life photo of the IoT-Chip demo application with RFID Reader
  |   |     and LCD Display
  |   |
  |   +- IoTChip_MQTT_WebClient_IpConfiguration.png
  |         IP Address configuration scheme for OpenPCS / PLC sample project
  |         'IoTChip_RFID_LCD_MQTT' (see above)
  |         (correlation of IP address configuration between IoT-Chip,
  |         MQTT broker server 'Mosquitto' and Web client)
  |
  +- Reference Schematics
  |         Reference Schematics of IoT-Chip Application Board
  |
  +- USB-RS232
  |         USB-RS232 Driver for CP210x from Silabs
  |         (This driver allows for the connection of serial interface COM0
  |          of IoT-Chip with the maintinace PC, tunneled via USB)
  |
  + EDS File
  |         EDS-File for CANopen tools
  |
  +- Manuals
      |
      +- L-1966e_01 System Manual IoT-Chip.pdf
      |     System Manual IoT-Chip
      |
      +- L-1007e_03 OpenPCS Quick-Start Instructions
      |     OpenPCS Quick-Start Instructions
      |
      +- L-1054e_05 SysExt.pdf
      |     SYS TEC-specific Extensions for OpenPCS / IEC 61131-3
      |
      +- L-1008e_07 Cop1131.pdf
      |     CAN / CANopen Extension for IEC 61131-3
      |
      +- L-1829e_01 FBLibModbus.pdf
            SYS TEC-specific Modbus Function Block Library for OpenPCS




