USB-RS232-adapter CD v3.0 Release Notes

This release contains the following components:

* Driver  
* Readme.txt (this file)
* Documentation directory
	* AN197: Serial Communications Guide for CP210x from Silabs
* Software directory
	* CP210xSerialTest: Serial Communications Sample Software from Silabs
	* CP210xPortNumExample: Serial Communications Port Num Sample Software from Silabs

Driver Installation
-------------------

	Follow the steps below to uninstall previous driver versions
	and to install the new drivers included in this package. See 
	the User's Guide for further driver installation instructions. 


	1) Unplug any connected USB-RS232-adapter.
	2) Remove old drivers that have previously been installed. 
	   For Windows systems, open the Add or Remove Programs 
	   window from the Control Panel. Next, select each CP210x
	   entry and click on Remove.
	3) Connect a CP210x device.
	4) Install the new drivers. For Windows systems, the Add New 
	   Hardware Wizard should open when a new device is detected. 
	   Use the wizard to install the drivers by directing it to 
	   the "\SO-1080\Drivers\Windows_XP_S2K3_Vista_7" directory" 
	   located on the CD. 
	5) See the User's Guide for further driver
	   installation instructions.


Known Issues and Limitations
----------------------------

	This driver release package includes the following drivers:
		* CP210x Linux VCP Driver v3.1
		* CP210x Macintosh OSX Driver v2.9
		* CP210x Windows XP/2003/Vista(32/64)/7(32/64) Driver v6.5
		* CP210x Windows 2000 Driver v6.3a
        * CP210x WinCE 5.0 VCP Driver  2.1
        * CP210x WinCE 6.0 VCP Driver  2.1
        
USB-RS232-adapter CD Revision History
-------------------------------------


Version 3.0
	
	Initial Release


